**Assembly File**

1. Fix C-clip positions fully
2. Add feet to the bottom of the legs

**Final Product Considerations**

1. Increase the horizontal spacing between the legs (can be closer to the walls most likely) to improve stability
2. Find better way to affix top sliding rod to the box